wguide2
Prev | Orchestra Opcodes and Operators | Next

## wguide2

wguide2 — A model of beaten plate consisting of two parallel delay-lines and two first-order lowpass filters.

## Description

A model of beaten plate consisting of two parallel delay-lines and two first-order lowpass filters.

## Syntax

    ares wguide2 asig, xfreq1, xfreq2, kcutoff1, kcutoff2, \
          kfeedback1, kfeedback2

## Performance

asig -- the input of excitation noise

xfreq1, xfreq2 -- the frequency (i.e. the inverse of delay time) Changed to x-rate in Csound version 3.59.

kcutoff1, kcutoff2 -- the filter cutoff frequency in Hz.

kfeedback1, kfeedback2 -- the feedback factor

wguide2 is a model of beaten plate consisting of two parallel delay-lines and two first-order lowpass filters. The two feedback lines are mixed and sent to the delay again each cycle.

Implementing waveguide algorithms as opcodes, instead of orc instruments, allows the user to set kr different than sr, allowing better performance particulary when using real-time.

wguide2.

| Note
As a rule of thumb, to avoid making wguide2 unstable, the sum of the two feedback values should be below 0.5.

## Examples

Here is an example of the wguide2 opcode. It uses the file wguide2.csd.

Example 584. Example of the wguide1 opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d     ;;;RT audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; -o wguide1.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>
    sr = 44100
    nchnls = 2
    instr 1
      afrq  line    50, 10, 100
      asig  oscil   3000, afrq, 1
      aenv  expon   1,10,0.000001
      aexc  =       aenv*asig
      ares  wguide2 aexc, 500, 1200, 777, 1500, 0.2, 0.25
            out ares,asig
    endin
    </CsInstruments>
    <CsScore>
    f1 0 4096 10 1
    i1 0 3
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

wguide1

## Credits

Author: Gabriel Maldonado
Italy
October 1998

New in Csound version 3.49

Example written by John ffitch

Prev | Up | Next
wguide1 | Home | wrap