pvscross
Prev | Orchestra Opcodes and Operators | Next

## pvscross

pvscross — Performs cross-synthesis between two source fsigs.

## Description

Performs cross-synthesis between two source fsigs.

## Syntax

    fsig pvscross fsrc, fdest, kamp1, kamp2

## Performance

The operation of this opcode is identical to that of pvcross (q.v.), except in using fsigs rather than analysis files, and the absence of spectral envelope preservation. The amplitudes from fsrc and fdest (using scale factors kamp1 for fsrc and kamp2 for fdest) are applied to the frequencies of fsrc. kamp1 and kamp2 must not exceed the range 0 to 1.

With this opcode, cross-synthesis can be performed on real-time audio input, by using pvsanal to generate fsrc and fdest. These must have the same format.

| Warning
It is unsafe to use the same f-variable for both input and output of pvs opcodes. Using the same one might lead to undefined behavior on some opcodes. Use a different one on the left and right sides of the opcode.

## Examples

    kcross  linseg    0,p3/3,0,p3/3,1,p3/3,1 ; progressive cross-synthesis
    fcross  pvscross  fsig1,fsig2,1-kcross,kcross
    across  pvsynth   fcross

## Credits

Author: Richard Dobson
August 2001

November 2003. Thanks to Kanata Motohashi, fixed the link to the pvcross opcode.

New in version 4.13

Prev | Up | Next
pvscent | Home | pvsdemix