Signal Input
Prev | Signal Input and Output | Next

## Signal Input

The opcodes that receive audio signals are:

- Synchronous input: in, in32, inch, inh, ino, inq, inrg, ins and inx

- File streaming: diskin, diskin2 and soundin

- User defined channel input: invalue

- Streaming input: soundin

- Direct to zak input: inz

See the section Software Bus for input and output through the API.

Prev | Up | Next
Signal Input and Output | Home | Signal Output