<CsoundSynthesizer>
<CsOptions>
; Select audio/midi flags here according to platform
; Audio out   Audio in
-odac           -iadc    ;;;RT audio I/O
; For Non-realtime ouput leave only the line below:
; -o gen06.wav -W ;;; for file output any platform
</CsOptions>
<CsInstruments>

; Initialize the global variables.
sr = 44100
kr = 4410
ksmps = 10
nchnls = 1

; Instrument #1.
instr 1
  ; Create an index over the length of our entire note.
  kcps init 1/p3
  kndx phasor kcps

  ; Read Table #1 with our index.
  ifn = 1
  ixmode = 1
  kval table kndx, ifn, ixmode

  ; Generate a sine waveform, use our Table #1 value to 
  ; vary its frequency by 100 Hz from its base frequency.
  ibasefreq = 440
  kfreq = kval * 100
  a1 oscil 20000, ibasefreq + kfreq, 2
  out a1
endin


</CsInstruments>
<CsScore>

; Table #1: a curve (using GEN06).
f 1 0 65 6 0 16 0.5 16 1 16 0 16 -1
; Table #2, a sine wave.
f 2 0 16384 10 1

; Play Instrument #1 for 2 seconds.
i 1 0 2
e


</CsScore>
</CsoundSynthesizer>
