ampmidi
Prev | Orchestra Opcodes and Operators | Next

## ampmidi

ampmidi — Get the velocity of the current MIDI event.

## Description

Get the velocity of the current MIDI event.

## Syntax

    iamp ampmidi iscal [, ifn]

## Initialization

iscal -- i-time scaling factor

ifn (optional, default=0) -- function table number of a normalized translation table, by which the incoming value is first interpreted. The default value is 0, denoting no translation.

## Performance

Get the velocity of the current MIDI event, optionally pass it through a normalized translation table, and return an amplitude value in the range 0 - iscal.

## Examples

Here is an example of the ampmidi opcode. It uses the file ampmidi.csd.

Example 41. Example of the ampmidi opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in   No messages  MIDI in
    -odac           -iadc     -d         -M0  ;;;RT audio I/O with MIDI in
    ; For Non-realtime ouput leave only the line below:
    ; -o ampmidi.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ; Initialize the global variables.
    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 1

    ; Instrument #1.
    instr 1
      ; Scale the amplitude between 0 and 1.
      ; This example expects MIDI note inputs on channel 1
      i1 ampmidi 1

      print i1
    endin

    </CsInstruments>
    <CsScore>

    ;Dummy f-table to give time for real-time MIDI events
    f 0 8000
    e

    </CsScore>
    </CsoundSynthesizer>

## See Also

aftouch, cpsmidi, cpsmidib, midictrl, notnum, octmidi, octmidib, pchbend, pchmidi, pchmidib, veloc

## Credits

Author: Barry L. Vercoe - Mike Berry
MIT - Mills
May 1997

Example written by Kevin Conder.

Prev | Up | Next
ampdbfs | Home | apcauchy