Operations Between a Vectorial and a Scalar Signal
Prev | Vectorial Opcodes | Next

## Operations Between a Vectorial and a Scalar Signal

These opcodes perform numeric operations between a vectorial control signal (hosted inside a function table), and a scalar signal. Result is a new vector that overrides old values of the table. There are k-rate and i-rate versions of the opcodes.

All these operators are designed to be used together with other opcodes that operate with vectorial signals such as bmscan, vcella, adsynt, adsynt2 etc.

Operations Between a Vectorial and a Scalar Signal:

- vadd

- vmult

- vpow

- vexp

- vadd_i

- vmult_i

- vpow_i

- vexp_i

Prev | Up | Next
Vectorial Opcodes | Home | Operations Between two Vectorial Signals