pvsmorph
Prev | Orchestra Opcodes and Operators | Next

## pvsmorph

pvsmorph — Performs morphing (or interpolation) between two source fsigs.

## Description

Performs morphing (or interpolation) between two source fsigs.

## Syntax

    fsig pvsmorph fsig1, fsig2, kampint, kfrqint

## Performance

The operation of this opcode is similar to that of pvinterp (q.v.), except in using fsigs rather than analysis files, and the absence of spectral envelope preservation. The amplitudes and frequencies of fsig1 are interpolated witht those of fsig2, depeding on the values of kampint and kfrqint, respectively. These range between 0 and 1, where 0 means fsig1 and 1, fsig2. Anything in between will interpolate amps and/or freqs of the two fsigs.

With this opcode, morphing can be performed on real-time audio input, by using pvsanal to generate fsig1 and fsig2. These must have the same format.

| Warning
It is unsafe to use the same f-variable for both input and output of pvs opcodes. Using the same one might lead to undefined behavior on some opcodes. Use a different one on the left and right sides of the opcode.

## Examples

              km  linseg    0,p3/3,0,p3/3,1,p3/3,1 ; progressive morphing
              fmo  pvsmorph  fsig1,fsig2,km,km
              asig  pvsynth   fmo

## Credits

Author: Victor Lazzarini
April 2007

New in Csound 5.06

Prev | Up | Next
pvsmix | Home | pvsmooth