midic14
Prev | Orchestra Opcodes and Operators | Next

## midic14

midic14 — Allows a floating-point 14-bit MIDI signal scaled with a minimum and a maximum range.

## Description

Allows a floating-point 14-bit MIDI signal scaled with a minimum and a maximum range.

## Syntax

    idest midic14 ictlno1, ictlno2, imin, imax [, ifn]

    kdest midic14 ictlno1, ictlno2, kmin, kmax [, ifn]

## Initialization

idest -- output signal

ictln1o -- most-significant byte controller number (0-127)

ictlno2 -- least-significant byte controller number (0-127)

imin -- user-defined minimum floating-point value of output

imax -- user-defined maximum floating-point value of output

ifn (optional) -- table to be read when indexing is required. Table must be normalized. Output is scaled according to imin and imax values.

## Performance

kdest -- output signal

kmin -- user-defined minimum floating-point value of output

kmax -- user-defined maximum floating-point value of output

midic14 (i- and k-rate 14 bit MIDI control) allows a floating-point 14-bit MIDI signal scaled with a minimum and a maximum range. The minimum and maximum values can be varied at k-rate. It can use optional interpolated table indexing. It requires two MIDI controllers as input.

| Note
Please note that the midic family of opcodes are designed for MIDI triggered events, and don't require a channel number since they will respond to the same channel as the one that triggered the instrument (see massign). However they will crash if called from a score driven event.

## See Also

ctrl7, ctrl14, ctrl21, initc7, initc14, initc21, midic7, midic21

## Credits

Author: Gabriel Maldonado
Italy

New in Csound version 3.47

Thanks goes to Rasmus Ekman for pointing out the correct controller number range.

Prev | Up | Next
metro | Home | midic21