JackoTransport
Prev | Orchestra Opcodes and Operators | Next

## JackoTransport

JackoTransport — Control the Jack transport.

## Description

Starts, stops, or repositions the Jack transport. This is useful, e.g., for starting an external sequencer playing to send MIDI messages to Csound.

## Syntax

    JackoTransport  kcommand, [kposition]

## Performance

kcommand -- 0 means "no action", 1 starts the transport, 2 stops the transport, and 3 positions the transport to kposition seconds from the beginning of performance (i.e. time 0 in the score).

kposition -- Time to position to the transport, in seconds from the beginning of performance (i.e. time 0 in the score).

This opcode can be used at init time or during performance.

The granularity of timing is Csound's kperiod.

## See Also

JackoInfo, JackoInfo, JackoFreewheel, JackoAudioOutConnect, JackoMidiInConnect, JackoMidiOutConnect, JackoOn, JackoAudioIn, JackoMidiOut, JackoNoteOut.

## Credits

By: Michael Gogins 2010

Prev | Up | Next
JackoOn | Home | jacktransport