Signal Input
Prev | Signal Input and Output | Next

## Signal Input

The opcodes that receive audio signals are:

- Synchronous input: in, in32, inch, inh, ino, inq, inrg, ins and inx

- File streaming: diskin, diskin2 and soundin

- User defined channel input: invalue

- Streaming input: soundin

- Direct to zak input: inz

See the section Software Bus for input and output through the API.

The mp3in allows reading of mp3 files, which are currently not supported by ordinary reading methods inside Csound.

Prev | Up | Next
Signal Input and Output | Home | Signal Output