wrap
Prev | Orchestra Opcodes and Operators | Next

## wrap

wrap — Wraps-around the signal that exceeds the low and high thresholds.

## Description

Wraps-around the signal that exceeds the low and high thresholds.

## Syntax

    ares wrap asig, klow, khigh

    ires wrap isig, ilow, ihigh

    kres wrap ksig, klow, khigh

## Initialization

isig -- input signal

ilow -- low threshold

ihigh -- high threshold

## Performance

xsig -- input signal

klow -- low threshold

khigh -- high threshold

wrap wraps-around the signal that exceeds the low and high thresholds.

This opcode is useful in several situations, such as table indexing or for clipping and modeling a-rate, i-rate or k-rate signals. wrap is also useful for wrap-around of table data when the maximum index is not a power of two (see table and tablei). Another use of wrap is in cyclical event repeating, with arbitrary cycle length.

## See Also

limit, mirror

## Credits

Author: Gabriel Maldonado
Italy

New in Csound version 3.49

Prev | Up | Next
wiisend | Home | wterrain