pvsmix
Prev | Orchestra Opcodes and Operators | Next

## pvsmix

pvsmix — Mix 'seamlessly' two pv signals.

## Description

Mix 'seamlessly' two pv signals. This opcode combines the most prominent components of two pvoc streams into a single mixed stream.

## Syntax

    fsig pvsmix fsigin1, fsigin2

## Performance

fsig -- output pv stream

fsigin1 -- input pv stream.

fsigin2 -- input pv stream, which must have same format as fsigin1.

| Warning
It is unsafe to use the same f-variable for both input and output of pvs opcodes. Using the same one might lead to undefined behavior on some opcodes. Use a different one on the left and right sides of the opcode.

## Examples

Example 488. Example

    fsig1	pvsanal  asig1,1024,256,1024,0  ; pvoc analysis
    fsig2   pvsanal  asig2,1024,256,1024,0
    fsigout	pvsmix  fsig1, fsig2         ; mix signals
    aout	pvsynth fsigout              ; pvoc synthesis

Depending on the input, this will transform a pitched sound into an inharmonic, bell-like sound.

## Credits

Author: Victor Lazzarini
November 2004

New plugin in version 5

Nivember 2004.

Prev | Up | Next
pvsmaska | Home | pvsmorph