outleta
Prev | Orchestra Opcodes and Operators | Next

## outleta

outleta — Sends an arate signal out from an instrument to a named port.

## Description

Sends an arate signal out from an instrument to a named port.

## Syntax

    outleta Sname, asignal

## Initialization

Sname -- String name of the outlet port. The name of the outlet is implicitly qualified by the instrument name or number, so it is valid to use the same outlet name in more than one instrument (but not to use the same outlet name twice in one instrument).

## Performance

asignal -- audio output signal

During performance, the audio output signal is sent to each instance of an instrument containing an inlet port to which this outlet has been connected using the connect opcode. The signals of all the outlets connected to an inlet are summed in the inlet.

## See Also

outletk outletf inleta inletk inletf connect alwayson ftgenonce

## Credits

By: Michael Gogins 2009

Prev | Up | Next
outkpc | Home | outletk