lpf18
Prev | Orchestra Opcodes and Operators | Next

## lpf18

lpf18 — A 3-pole sweepable resonant lowpass filter.

## Description

Implementation of a 3 pole sweepable resonant lowpass filter.

## Syntax

    ares lpf18 asig, kfco, kres, kdist

## Performance

kfco -- the filter cutoff frequency in Hz. Should be in the range 0 to sr/2.

kres -- the amount of resonance. Self-oscillation occurs when kres is approximately 1. Should usually be in the range 0 to 1, however, values slightly greater than 1 are possible for more sustained oscillation and an “overdrive” effect.

kdist -- amount of distortion. kdist = 0 gives a clean output. kdist > 0 adds tanh() distortion controlled by the filter parameters, in such a way that both low cutoff and high resonance increase the distortion amount. Some experimentation is encouraged.

lpf18 is a digital emulation of a 3 pole (18 dB/oct.) lowpass filter capable of self-oscillation with a built-in distortion unit. It is really a 3-pole version of moogvcf, retuned, recalibrated and with some performance improvements. The tuning and feedback tables use no more than 6 adds and 6 multiplies per control rate. The distortion unit, itself, is based on a modified tanh function driven by the filter controls.

| Note
This filter requires that the input signal be normalized to one.

## Examples

Here is an example of the lpf18 opcode. It uses the file lpf18.csd.

Example 350. Example of the lpf18 opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d     ;;;RT audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; -o lpf18.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ; Initialize the global variables.
    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 1

    ; Instrument #1.
    instr 1
      ; Generate a sine waveform.
      ; Note that its amplitude (kamp) ranges from 0 to 1.
      kamp init 1
      kcps init 440
      knh init 3
      ifn = 1
      asine buzz kamp, kcps, knh, ifn

      ; Filter the sine waveform.
      ; Vary the cutoff frequency (kfco) from 300 to 3,000 Hz.
      kfco line 300, p3, 3000
      kres init 0.8
      kdist = p4
      ivol = p5
      aout lpf18 asine, kfco, kres, kdist

      out aout * ivol
    endin

    </CsInstruments>
    <CsScore>

    ; Table #1, a sine wave.
    f 1 0 16384 10 1

    ; different distortion and volumes to compensate
    i 1 0 4 0.2 30000
    i 1 4.5 4 0.9 27000
    e

    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: Josep M Comajuncosas
Spain
December 2000

Example written by Kevin Conder with help from Iain Duncan. Thanks goes to Iain for helping with the example.

New in Csound version 4.10

Prev | Up | Next
lowresx | Home | lpfreson