ATSpartialtap
Prev | Orchestra Opcodes and Operators | Next

## ATSpartialtap

ATSpartialtap — returns a frequency, amplitude pair from an ATSbufread opcode.

## Description

ATSpartialtap takes a partial number and returns a frequency, amplitude pair. The frequency and amplitude data comes from an ATSbufread opcode.

## Syntax

    kfrq, kamp ATSpartialtap ipartialnum

## Initialization

ipartialnum - indicates the partial that the ATSpartialtap opcode should read from an ATSbufread.

## Performance

kfrq - returns the frequency value for the requested partial.

kamp - returns the amplitude value for the requested partial.

ATSpartialtap takes a partial number and returns a frequency, amplitude pair. The frequency and amplitude data comes from an ATSbufread opcode. This is more restricted version of ATSread, since each ATSread opcode has its own independent time pointer, and ATSpartialtap is restricted to the data given by an ATSbufread. Its simplicity is its attractive feature.

## Examples

Here is an example of the ATSpartialtap opcode. It uses the file ATSpartialtap.csd.

Example 60. Example of the ATSpartialtap opcode.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;RT audio out
    ;-iadc    ;;;uncomment -iadc for RT audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o ATSpartialtap.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs = 1

    instr 1	; "beats.ats" is created by atsa

    ktime	line	0, p3, 2
    	ATSbufread ktime, 1, "beats.ats", 30
    kfreq1, kam1	ATSpartialtap  5
    kfreq2, kam2	ATSpartialtap  20
    kfreq3, kam3	ATSpartialtap  30

    aout1	oscil	kam1, kfreq1, 1
    aout2	oscil	kam2, kfreq2, 1
    aout3	oscil	kam3, kfreq3, 1
    aout	=	(aout1+aout2+aout3)*10	; amplify some more
    	outs	aout, aout

    endin

    </CsInstruments>
    <CsScore>
    ; sine wave.
    f 1 0 16384 10 1
    i 1 0 2
    e

    </CsScore>
    </CsoundSynthesizer>

This example here uses an ATSpartialtap, and an ATSbufread to read partials 5, 20 and 30 from 'beats.ats'. These amplitudes and frequencies could be used to re-synthesize those partials, or something all together different.

## See also

ATSread, ATSreadnz, ATSinfo, ATSsinnoi, ATSbufread, ATScross, ATSinterpread, ATSadd, ATSaddnz

## Credits

Author: Alex Norman
Seattle,Washington
2004

Prev | Up | Next
ATSreadnz | Home | ATSsinnoi