pvsin
Prev | Orchestra Opcodes and Operators | Next

## pvsin

pvsin — Retrieve an fsig from the input software bus; a pvs equivalent to chani.

## Description

This opcode retrieves an f-sig from the pvs in software bus, which can be used to get data from an external source, using the Csound 5 API. A channel is created if not already existing. The fsig channel is in that case initialised with the given parameters. It is important to note that the pvs input and output (pvsout opcode) busses are independent and data is not shared between them.

## Syntax

    fsig pvsin kchan[,isize,iolap,iwinsize,iwintype,iformat]

## Initialisation

isize -- initial DFT size,defaults to 1024.

iolap -- size of overlap, defaults to isize/4.

isize -- size of analysis window, defaults to isize.

isize -- type of window, defaults to Hanning (1) (see pvsanal)

isize -- data format, defaults 0 (PVS_AMP_FREQ). Other possible values are 1 (PVS_AMP_PHASE), 2 (PVS_COMPLEX) or 3 (PVS_TRACKS).

## Performance

fsig -- output fsig.

kchan -- channel number. If non-existent, a channel will be created.

## Examples

Example 485. Example

              fsig  pvsin   0 ; get data from pvs in bus channel 0

## Credits

Author: Victor Lazzarini
Auust 2006

Prev | Up | Next
pvsinit | Home | pvslock