wiisend
Prev | Orchestra Opcodes and Operators | Next

## wiisend

wiisend — Sends data to one of a number of external Nintendo Wiimote controllers.

## Description

Sends data to one of a number of external Nintendo Wiimote controllers.

## Syntax

    kres wiisend kcontrol, kvalue[, knum]

## Initialization

This opcode must be used in conjuction with a running wiiconnect opcode.

## Performance

| Note
Please note that these opcodes are currently only supported on Linux.

kcontrol -- the code for which control to write.

kvalue -- the value to write to the control.

knum -- the number of the which Wiimote to access, which defaults to the first one (zero).

On each access a particular data item of the Wiimote is written. The currently implemented controls are given below, together with the macro name defined in the file wii_mac:

3 (WII_RUMBLE): starts or stops the Wiimote rumbling, depending on the value of kvalue (0 to stop, 1 to start).

4 (WII_SET_LEDS): set the four LED lights on the Wiimote to the binary representation of kvalue.

## Examples

See the example for wiiconnect.

## See Also

wiiconnect, wiidata, wiirange,

## Credits

Author: John ffitch
Codemist Ltd
2009

New in version 5.11

Prev | Up | Next
wiirange | Home | wrap