vmult_i
Prev | Orchestra Opcodes and Operators | Next

## vmult_i

vmult_i — Multiplies a vector in a table by a scalar value.

## Description

Multiplies a vector in a table by a scalar value.

## Syntax

    vmult_i  ifn, ival, ielements [, idstoffset]

## Initialization

ifn - number of the table hosting the vectorial signal to be processed

ival - scalar value to be multiplied

ielements - number of elements of the vector

idstoffset - index offset for the destination table

## Performance

vmult_i multiplies each element of the vector contained in the table ifn by ival, starting from table index idstoffset. This enables you to process a specific section of a table by specifying the offset and the number of elements to be processed. Offset is counted starting from 0, so if no offset is specified (or set to 0), the table will be modified from the beginning.

This opcode runs only on initialization, there is a k-rate version of this opcode called vmult.

Negative values for idstoffset are valid. Elements from the vector that are outside the table, will be discarded, and they will not wrap around the table.

In all these opcodes, the resulting vectors are stored in ifn, overriding the intial vectors. If you want to keep initial vector, use vcopy or vcopy_i to copy it in another table. All these operators are designed to be used together with other opcodes that operate with vectorial signals such as bmscan, vcella, adsynt, adsynt2, etc. They can also be useful in conjunction with the spectral opcodes pvsftw and pvsftr.

## Examples

Here is an example of the vmult_i opcode. It uses the file vmult_i.csd.

Example 892. Example of the vmult_i opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in
    -odac           -iadc     ;;;RT audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; -o cigoto.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr=44100
    ksmps=128
    nchnls=2

    	instr 1
    ifn1 = p4
    ival = p5
    ielements = p6
    idstoffset = p7
    kval init 25
    vmult_i ifn1, ival, ielements, idstoffset
    	endin

    	instr 2	;Printtable
    itable = p4
    isize = ftlen(itable)
    kcount init 0
    kval table kcount, itable
    printk2 kval

    if (kcount == isize) then
      turnoff
    endif

    kcount = kcount + 1
    	endin

    </CsInstruments>
    <CsScore>

    f 1 0 16 -7 1 16 17

    i2	0.0	0.2	1
    i1	0.4	0.01	1	2	3	4
    i2	0.8	0.2	1
    i1	1.0	0.01	1	0.5	5	-3
    i2	1.2	0.2	1
    i1	1.4	0.01	1	1.5	10	12
    i2	1.6	0.2	1
    e

    </CsScore>
    </CsoundSynthesizer>

## See also

vadd, vadd, vmult, vpow_i, vpow, vexp_i and vexp.

## Credits

Written by Gabriel Maldonado. Optional arguments added by Andres Cabrera and Istvan Varga.

Example by Andres Cabrera.

New in Csound 5 (Previously available only on CsoundAV)

Prev | Up | Next
vmult | Home | vmultv