rms
Prev | Orchestra Opcodes and Operators | Next

## rms

rms — Determines the root-mean-square amplitude of an audio signal.

## Description

Determines the root-mean-square amplitude of an audio signal. It low-pass filters the actual value, to average in the manner of a VU meter.

## Syntax

    kres rms asig [, ihp] [, iskip]

## Initialization

ihp (optional, default=10) -- half-power point (in Hz) of a special internal low-pass filter. The default value is 10.

iskip (optional, default=0) -- initial disposition of internal data space (see reson). The default value is 0.

## Performance

asig -- input audio signal

kres -- low-pass filtered rms value of the input signal

rms output values kres will trace the root-mean-square value of the audio input asig. This unit is not a signal modifier, but functions rather as a signal power-gauge. It uses an internal low-pass filter to make the response smoother. ihp can be used to control this smoothing. The higher the value, the "snappier" the measurement.

This opcode can also be used as an evelope follower.

The kres output from this opcode is given in amplitude and depends on 0dbfs. If you want the output in decibels, you can use dbamp

## Examples

    arms rms    asig ; get rms value of signal asig

Here is an example of the rms opcode. It uses the file rms.csd.

Example 695. Example of the rms opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d  -m0   ;;;RT audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; -o rms.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ; Initialize the global variables.
    sr = 44100
    ksmps = 128
    nchnls = 1

    ;Example by Andres Cabrera 2007

    0dbfs = 1

    FLpanel "rms", 400, 100, 50, 50
        gkrmstext, gihrmstext FLtext "Rms", -100, 0, 0.1, 3, 110, 30, 60, 50
        gkihp, gihandle FLtext "ihp", 0, 10, 0.05, 1, 100, 30, 220, 50
        gkrmsslider, gihrmsslider FLslider "", -60, -0.5, -1, 5, -1, 380, 20, 10, 10

    FLpanelEnd
    FLrun

    FLsetVal_i 5, gihandle
    ; Instrument #1.
    instr 1
      a1 inch 1

    label:
      kval rms a1, i(gkihp)  ;measures rms of input channel 1
    rireturn

      kval = dbamp(kval) ; convert to db full scale
      printk 0.5, kval
      FLsetVal 1, kval, gihrmsslider   ;update the slider and text values
      FLsetVal 1, kval, gihrmstext
      knewihp changed gkihp   ; reinit when ihp text has changed
      if (knewihp == 1) then
        reinit label  ;needed because ihp is an i-rate parameter
      endif
    endin

    </CsInstruments>
    <CsScore>

    ; Play Instrument #1 for one minute
    i 1 0 60
    e

    </CsScore>
    </CsoundSynthesizer>

## See Also

balance, gain

Prev | Up | Next
rireturn | Home | rnd