dssictls
Prev | Orchestra Opcodes and Operators | Next

## dssictls

dssictls — Send control information to a LADSPA or DSSI plugin.

## Syntax

    dssictls ihandle, iport, kvalue, ktrigger

## Description

dssictls sends control values to a plugin's control port

## Initialization

ihandle - handle for the plugin returned by dssiinit

iport - control port number

## Performance

kvalue - value to be assigned to the port

ktrigger - determines whether the control information will be sent (ktrigger = 1) or not. This is useful for thinning control information, generating ktrigger with metro

dssictls sends control information to a LADSPA or DSSI plugin's control port. The valid control ports and ranges are given by dssiinit . Using values outside the ranges may produce unspecified behaviour.

## Examples

Here is an example of the dssictls opcode. It uses the file dssictls.csd.

Example 186. Example of the dssictls opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;RT audio out
    ;-iadc    ;;;uncomment -iadc if RT audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o dssictls.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2

    gihandle dssiinit "caps.so", 1, 1	; = equaliser and
    gaoutl init  0				; verbose about all ports
    gaoutr init  0

    instr 1	; activate DSSI

    dssiactivate gihandle, 1
    endin

    instr 2
    ain1	diskin2 "beats.wav", 1,0,1	; loop

    gaoutl = gaoutl+(ain1*.1)		; temper input
    gaoutr = gaoutr+(ain1*.1)
    endin

    instr 3

    dssictls gihandle, 2, -48, 1	; 31 Hz range -48 to 24
    dssictls gihandle, 3, -48, 1	; 63 Hz range -48 to 24
    dssictls gihandle, 4, -48, 1	; 125 Hz range -48 to 24
    dssictls gihandle, 5, 20, 1	; 250 Hz range -48 to 24
    dssictls gihandle, 6, -48, 1	; 500 Hz range -48 to 24
    dssictls gihandle, 7, -48, 1	; 1 kHz Hz range -48 to 24
    dssictls gihandle, 8, -48, 1	; 2 kHz range -48 to 24
    dssictls gihandle, 9, 24, 1	; 4 kHz range -48 to 24
    dssictls gihandle, 10, 24, 1	; 8 kHz range -48 to 24
    dssictls gihandle, 11, 24, 1	; 16 kHz range -48 to 24

    endin

    instr 4

    aout1, aout2	dssiaudio gihandle, gaoutl, gaoutr	;get beats.wav, mono out
    		outs aout1,aout2

    gaoutl = 0
    gaoutr = 0
    endin

    </CsInstruments>
    <CsScore>
    i 1 0 20
    i 2 1 20
    i 3 1 20
    i 4 0 20

    e
    </CsScore>
    </CsoundSynthesizer>

## Credits

2005

By: Andrés Cabrera

Uses code from Richard Furse's LADSPA sdk.

Prev | Up | Next
dssiaudio | Home | dssiinit