inletk
Prev | Orchestra Opcodes and Operators | Next

## inletk

inletk — Receives a krate signal into an instrument from a named port.

## Description

Receives a krate signal into an instrument from a named port.

## Syntax

    ksignal inletk Sname

## Initialization

Sname -- String name of the inlet port. The name of the inlet is implicitly qualified by the instrument name or number, so it is valid to use the same inlet name in more than one instrument (but not to use the same inlet name twice in one instrument).

## Performance

ksignal -- krate input signal

During performance, the krate inlet signal is received from each instance of an instrument containing an outlet port to which this inlet has been connected using the connect opcode. The signals of all the outlets connected to an inlet are summed in the inlet.

## Examples

Here is an example of the inletk opcode. It uses the file inletk.csd.

Example 361. Example of the inletk opcode.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o inletk.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    connect "bend", "bendout", "guitar", "bendin"

    instr bend

    kbend line p4, p3, p5
          outletk "bendout", kbend
    endin

    instr guitar

    kbend inletk "bendin"
    kpch pow 2, kbend/12
         printk2 kpch
    asig oscili .4, 440*kpch, 1
         outs asig, asig
    endin

    </CsInstruments>
    <CsScore>

    f1 0 1024 10 1

    i"guitar" 0 5 8.00
    i"bend" 3 .2 -12 12
    i"bend" 4 .1 -17 40
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

outleta outletk outletkid outletf inleta inletf connect alwayson ftgenonce

## Credits

By: Michael Gogins 2009

Prev | Up | Next
inleta | Home | inletkid