outic
Prev | Orchestra Opcodes and Operators | Next

## outic

outic — Sends MIDI controller output at i-rate.

## Description

Sends MIDI controller output at i-rate.

## Syntax

    outic ichn, inum, ivalue, imin, imax

## Initialization

ichn -- MIDI channel number (1-16)

inum -- controller number (0-127 for example 1 = ModWheel; 2 = BreathControl etc.)

ivalue -- floating point value

imin -- minimum floating point value (converted in MIDI integer value 0)

imax -- maximum floating point value (converted in MIDI integer value 127 (7 bit))

## Performance

outic (i-rate MIDI controller output) sends controller messages to the MIDI OUT device. It works only with MIDI instruments which recognize them. It can drive a different value of a parameter for each note currently active.

It can scale an i-value floating-point argument according to the imin and imax values. For example, set imin = 1.0 and imax = 2.0. When the ivalue argument receives a 2.0 value, the opcode will send a 127 value to the MIDI OUT device. When the ivalue argument receives a 1.0 value, it will send a 0 value. i-rate opcodes send their message once during instrument initialization.

## Examples

Here is an example of the outic opcode. It uses the file outic.csd.

Example 537. Example of the outic opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac  -Q1 -M0  ;;;realtime audio out -+rtmidi=virtual
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o outic.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2

    instr 1

    ikey notnum
    ivel veloc
    kbrt = 40			;set controller 74 (=brightness)
    outic 1, 74, kbrt, 0, 127	;so filter closes a bit
    midion 1, ikey, ivel		;play external synth

    endin
    </CsInstruments>
    <CsScore>
    f0 30	;runs 30 seconds

    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

outiat, outic14, outipat, outipb, outipc, outkat, outkc14, outkc, outkpat, outkpb, outkpc

## Credits

Author: Gabriel Maldonado
Italy

New in Csound version 3.47

Thanks goes to Rasmus Ekman for pointing out the correct MIDI channel and controller number ranges.

Prev | Up | Next
outic14 | Home | outipat