vdelayxws
Prev | Orchestra Opcodes and Operators | Next

## vdelayxws

vdelayxws — Variable delay opcodes with high quality interpolation.

## Description

Variable delay opcodes with high quality interpolation.

## Syntax

    aout1, aout2 vdelayxws ain1, ain2, adl, imd, iws [, ist]

## Initialization

imd -- max. delay time (seconds)

iws -- interpolation window size (see below)

ist (optional) -- skip initialization if not zero

## Performance

ain1, ain2 -- input audio signals

aout1, aout2 -- output audio signals

adl -- delay time in seconds

These opcodes use high quality (and slow) interpolation, that is much more accurate than the currently available linear and cubic interpolation. The iws parameter sets the number of input samples used for calculating one output sample (allowed values are any integer multiply of 4 in the range 4 - 1024); higher values mean better quality and slower speed.

The vdelayxw opcodes change the position of the write tap in the delay line (unlike all other delay ugens that move the read tap), and are most useful for implementing Doppler effects where the position of the listener is fixed, and the sound source is moving.

The multichannel opcodes (eg. vdelayxq) allow delaying 2 or 4 variables at once (stereo or quad signals); this is much more efficient than using separate opcodes for each channel.

| Notes
Delay time is measured in seconds (unlike in vdelay and vdelay3), and must be a-rate. The minimum allowed delay is iws/2 samples. Using the same variables as input and output is allowed in these opcodes. In vdelayxw*, changing the delay time has some effects on output volume: a = 1 / (1 + dt) where a is the output gain, and dt is the change of delay time per seconds. These opcodes are best used in the double-precision version of Csound.

## Examples

Here is an example of the use of the vdelayxws opcode. It uses the file vdelayxws.csd.

Example 921. Example of the vdelayxws opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac  ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o vdelayxws.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    ims  =	.5						;maximum delay time in seconds
    iws  =	1024						;window size
    adl  =	.5						;delay time
    asig1, asig2 diskin2 "kickroll.wav", 1, 0, 1		;loop stereo file kickroll.wav
    a2   poscil .2, .1, 1					;make an LFO, 1 cycle per 10 seconds
    adl  = a2 + ims/2      					;offset the LFO so that it is positive
    aoutL, aoutR vdelayxws asig1, asig2, adl, ims, iws	;use the LFO to control delay time
         outs aoutL, aoutR

    endin
    </CsInstruments>
    <CsScore>
    f1 0 8192 10 1

    i 1 0 10

    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

vdelayx, vdelayxq, vdelayxs, vdelayxw, vdelayxwq

Prev | Up | Next
vdelayxwq | Home | vdivv