<CsoundSynthesizer>
<CsOptions>
; Select audio/midi flags here according to platform
; Audio out   Audio in    No messages
-odac           -iadc     -d     ;;;RT audio I/O
; For Non-realtime ouput leave only the line below:
; -o lpread.wav -W ;;; for file output any platform
</CsOptions>
<CsInstruments>

; Initialize the global variables.
sr = 44100
kr = 4410
ksmps = 10
nchnls = 1

; Instrument #1.
instr 1
;can use -a option when analyzing (= filter coefficient) or without -a option "fox.wav" from the manual
;fox.lpc = 2.8 seconds long
ktime  line 0, p3, 2.8       ; Define time lin
krmsr,krmso,kerr,kcps lpread    ktime,"foxpoles.lp"
aout	buzz	krmso, kcps, 15, 1
asig	rand	krmsr

       out aout*2+asig


endin


</CsInstruments>
<CsScore>

f1 0 4096 10 1 

i 1 0 2.8
e


</CsScore>
</CsoundSynthesizer>
