pvsfilter
Prev | Orchestra Opcodes and Operators | Next

## pvsfilter

pvsfilter — Multiply amplitudes of a pvoc stream by those of a second pvoc stream, with dynamic scaling.

## Description

Multiply amplitudes of a pvoc stream by those of a second pvoc stream, with dynamic scaling.

## Syntax

    fsig pvsfilter fsigin, fsigfil, kdepth[, igain]

## Performance

fsig -- output pv stream

fsigin -- input pv stream.

fsigfil -- filtering pvoc stream.

kdepth -- controls the depth of filtering of fsigin by fsigfil .

igain -- amplitude scaling (optional, defaults to 1).

Here the input pvoc stream amplitudes are modified by the filtering stream, keeping its frequencies intact. As usual, both signals have to be in the same format.

| Warning
It is unsafe to use the same f-variable for both input and output of pvs opcodes. Using the same one might lead to undefined behavior on some opcodes. Use a different one on the left and right sides of the opcode.

## Examples

Example 625. Example

    kfreq  expon 500, p3, 4000           ; 3-octave sweep
    kdepth linseg 1, p3/2, 0.5, p3/2, 1  ; varying filter depth

    asig  in                             ; input
    afil  oscili  1, kfreq, 1            ; filter t-domain signal

    fim   pvsanal  asig,1024,256,1024,0  ; pvoc analysis
    fil   pvsanal  afil,1024,256,1024,0
    fou   pvsfilter fim, fil, kdepth     ; filter signal
    aout  pvsynth  fou                   ; pvoc synthesis

In the example above the filter curve will depend on the spectral envelope of afil; in the simple case of a sinusoid, it will be equivalent to a narrowband band-pass filter.

Here is an example of the use of the pvsfilter opcode. It uses the file pvsfilter.csd.

Example 626. Example of the pvsfilter opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    -odac
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 16
    nchnls = 1
    0dbfs = 1

    ;; example written by joachim heintz 2009

    giSine		ftgen		0, 0, 4096, 10, 1
    giBell		ftgen		0, 0, 4096, 9, .56, 1, 0, .57, .67, 0, .92, 1.8, 0, .93, 1.8, 0, 1.19, 2.67, 0, 1.7, 1.67, 0, 2, 1.46, 0, 2.74, 1.33, 0, 3, 1.33, 0, 3.76, 1, 0, 4.07, 1.33, 0; bell-like (after Risset)

    instr 1
    ipermut	=		p4; 1 = change order of soundfiles
    ifftsize	=		1024
    ioverlap	=		ifftsize / 4
    iwinsize	=		ifftsize
    iwinshape	=		1; von-Hann window
    Sfile1		=		"fox.wav"
    ain1		soundin	Sfile1
    kfreq		randomi	200, 300, 3
    ain2		oscili		.2, kfreq, giBell
    ;ain2		oscili		.2, kfreq, giSine; try also this
    fftin1		pvsanal	ain1, ifftsize, ioverlap, iwinsize, iwinshape; fft-analysis of file 1
    fftin2		pvsanal	ain2, ifftsize, ioverlap, iwinsize, iwinshape; fft-analysis of file 2
    if ipermut == 1 then
    fcross		pvsfilter	fftin2, fftin1, 1
    else
    fcross		pvsfilter	fftin1, fftin2, 1
    endif
    aout		pvsynth	fcross
    		out		aout * 20
    endin

    </CsInstruments>
    <CsScore>
    i 1 0 2.757 0; frequencies from fox.wav, amplitudes multiplied by amplitudes of giBell
    i 1 3 2.757 1; frequencies from giBell, amplitudes multiplied by amplitudes of fox.wav
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

pvsanal, pvsynth, pvsadsyn

## Credits

Author: Victor Lazzarini
November 2004

New plugin in version 5

November 2004.

Prev | Up | Next
pvsdisp | Home | pvsfread